**CORRIGENDUM**

**CONTRACT NOTICE**

**II.1.1) Contract Notice Title:** **Combined construction machine**
**II.1.1) Contract Notice Reference Number:** **RORS00239/Municipality of Golubac/TD1**

**VII. 1.1) Reason for change**

Modification of original information submitted by the contracting authority.

**VII.1.2) Text to be corrected in the original notice**

In

ANNEX II + III: TECHNICAL SPECIFICATIONS + TECHNICAL OFFER

Instead of:

| **1.****Item number** | **2.****Specifications required** | **3.****Specifications offered** | **4.****Notes, remarks, ref to documentation** | **5.****Evaluation committee’s notes**  |
| --- | --- | --- | --- | --- |
| **1** | **Combined construction machine**: 1 piece**Description and purpose of vehicle:** Combined backhoe loader/trencher**Engine power:** min 88 KW**Engine type:** diesel, STAGE V or better ecology standard**Engine Displacement**: max 3600cm3**Transmission**: 4WD **Supported steering modes:** 4WS, crab steering**Top speed road:** min 40 kmh**Operating Weight:** min 9.800kg**Tires size:** min 28”**Fuel capacity:** min 130l**Cabin protection from rolling over and falling objects in line with:*** Falling-object protective structures compliance
* Roll-over protective structures compliance

**Cabin Equipment:** AC device, radio**Hydraulic pump specifications:*** **Max working pressure:** less than 210 bar
* **Max flow:** min 165l/min

**Backhoe specifications:*** **Bucket width:** 600mm
* **Max Dig Depth:** min 5.8 meters
* **Max. loadover height (backhoe):** min 4m
* **Max Reach From Swivel:** min 5,8m
* Installation for possibility of mounting of pneumatic hammer
* Hydraulic coupler for quick attachments swap

**Loader specifications:*** **Bucket Capacity**: min 1,2 m3 type ”6 in 1”
* **Maximum lifting capacity at Max Dump Height:** min 3400 kg
* **Clearance at Max Dump Height**: min 2.7m
* **Reach at Max Dump Height**: min 0.7 m
* **Dig Depth**: min 80mm

**Aux Equipment:** * Combined construction machine is to be delivered with one additional 800mm and one 1500mm backhoe bucket (beside one 600mm already mounted on machine and mentioned above) as well one hydraulic hammer for backhoe mount.
* Alarm for reverse moving
* Rotation lights,
* Fire estinguiser in line with Serbian legislation,

**Important note**: Contractor must provide on-site training for two seasoned backhoe machine operators provided by Contracting Authority for handling and operation of machine after delivery is finished. |  |  |  |

Read:

| **1.****Item number** | **2.****Specifications required** | **3.****Specifications offered** | **4.****Notes, remarks, ref to documentation** | **5.****Evaluation committee’s notes**  |
| --- | --- | --- | --- | --- |
| **1** | **Combined construction machine**: 1 piece**Description and purpose of vehicle:** Combined backhoe loader/trencher**Engine power:** min 88 KW**Engine type:** diesel, STAGE V or better ecology standard**Engine Displacement**: max 3600cm3**Transmission**: 4WD **Supported steering modes:** 4WS, crab steering**Top speed road:** min 40 kmh**Operating Weight:** min 9.800kg**Tires size:** min 28”**Fuel capacity:** min 130l**Cabin protection from rolling over and falling objects in line with:*** Falling-object protective structures compliance
* Roll-over protective structures compliance

**Cabin Equipment:** AC device, radio**Hydraulic pump specifications:*** **Max working pressure:** less than 210 bar
* **Max flow:** min 165l/min

**Backhoe specifications:*** **Bucket width:** 600mm
* **Max Dig Depth:** min 5.8 meters
* **Max. loadover height (backhoe):** min 4m
* **Max Reach From Swivel:** min 5,8m
* Installation for possibility of mounting of pneumatic hammer
* Hydraulic coupler for quick attachments swap or mechanical quick coupler

**Loader specifications:*** **Bucket Capacity**: min 1,2 m3 type ”6 in 1”
* **Maximum lifting capacity at Max Dump Height:** min 3400 kg
* **Clearance at Max Dump Height**: min 2.7m
* **Reach at Max Dump Height**: min 0.7 m
* **Dig Depth**: min 80mm

**Aux Equipment:** * Combined construction machine is to be delivered with one additional 800mm and one 1500mm backhoe bucket (beside one 600mm already mounted on machine and mentioned above) as well one hydraulic hammer for backhoe mount.
* Alarm for reverse moving
* Rotation lights,
* Fire estinguiser in line with Serbian legislation,

**Important note**: Contractor must provide on-site training for two seasoned backhoe machine operators provided by Contracting Authority for handling and operation of machine after delivery is finished. |  |  |  |

All other terms and conditions of the contract notice remain unchanged. The above alterations and/or corrections to the contract notice are integral part of the contract notice.