# *ANNEX II + III:* TECHNICAL SPECIFICATIONS + TECHNICAL OFFER

**Contract title: Procurement of Water mobility means and Land mobility means for project "Safer climate within the Romanian-Serbian border Area - SAFE"**

**p 1 /…**

**Publication reference:** **RORS00004 - TD04/2**

**LOT no.2 - Land mobility means – Vehicle**

**Columns 1-2 should be completed by the contracting authority**

**Columns 3-4 should be completed by the tenderer**

**Column 5 is reserved for the evaluation committee**

Annex III - the contractor's technical offer

The tenderers are requested to complete the template on the next pages:

* Column 2 is completed by the contracting authority shows the required specifications (not to be modified by the tenderer),
* Column 3 is to be filled in by the tenderer and must detail what is offered (for example the words ‘compliant’ or ‘yes’ are not sufficient)
* Column 4 allows the tenderer to make comments on its proposed supply and to make eventual references to the documentation

The eventual documentation supplied should clearly indicate (highlight, mark) the models offered and the options included, if any, so that the evaluators can see the exact configuration. Offers that do not permit to identify precisely the models and the specifications may be rejected by the evaluation committee.

The offer must be clear enough to allow the evaluators to make an easy comparison between the requested specifications and the offeredspecifications.

**General Requirements**

• All requirements stated and outlined in this document must be regarded as mandatory and the minimum acceptable criteria. All requirements outlined in this document are accompanied by the phrase "or equivalent".

• The tenderer is required to provide the specifications of the offered items in the Technical Offer, including details such as the manufacturer, product type, model, and country of origin. All documentation must be provided in English or Serbian, both in hardcopy and electronic formats.

• The selected contractor is required to provide all necessary documentation for the registration of the completed vehicle in accordance with the relevant legal regulations in the Republic of Serbia. This includes the Certificate from the Agency for Traffic Safety confirming the vehicle examination, as well as the technical inspection registration sheet, which is required for further vehicle registration.

| **1.**  **Item number** | **2.**  **Specifications required** | **3.**  **Specifications offered** | **4.**  **Notes, remarks,  ref to documentation** | **5.**  **Evaluation committee’s notes** |
| --- | --- | --- | --- | --- |
| **1** | **4x4 Vehicle, Quantity: 5 Units** |  |  |  |
|  | **Main vehicle requirements**  - Delivered vehicles must be purchased from official importers or other legal entities that is expressly authorized by the manufacturer to deliver and maintain the offered vehicles.  - The vehicle must be left-hand drive,  - The vehicle must have 5 doors,  - The date of manufacture of the vehicle must not be older than 12 months from the date of delivery.  - Vehicle warranty for at least 4 years or 100,000 km  - The supplier must have a service network throughout the territory of the Republic of Serbia  **Technical requirements for vehicles**  - Type of vehicle intended for exploitation in off-road conditions,  - Clearance minimum 165mm  - Seats should provide: Ergonomic design, adjustable driver and passenger seat height  **Engine**  - The vehicle must have a four-stroke diesel or gasoline engine with water cooling.  - Minimum 1200cc - maximum 2000cc Engine power must not be less than 84 kw (115 KS),  - Gearbox: manual, semi-automatic or automatic.  **Drive system**  - Power transmission 4x4  - The vehicle must have a four-wheel drive system (permanent or variable).  - Optionally, the vehicle has a differential lock Braking system - the vehicle must have ABS, ASR, ESP. Optional Front assist, Lane assist,  Driver alert  **Additional equipment**  - The vehicle must be equipped with a set of steel (with wheel caps) or aluminum wheel minimum 16",  - An additional set of tires (with a note that they must be on them when handing over the vehicle tires for that season).  - The vehicle must be equipped with a spare wheel (parameters identical to those of ordinary ones seasonal wheels), lifting jack, wheel nut wrench,  - Safety kit (first aid not older than the vehicle's production date, triangle, gloves, reflective vest and cut. light bulbs)  - The vehicle must be equipped with at least two airbags - one for the driver and one for the passenger, optional side airbags.  - The vehicle must be equipped with three rear seat belts and three rear head restraints,  - Air conditioner  - The vehicle must be equipped with a central locking system with remote control  - Outside mirrors in the color of the vehicle  - Electric front and rear windows  - Electrically adjustable, heated and folding exterior mirrors with automatic dimming  - USB, socket 12 V,  - Interior mirror with automatic dimming and rain sensor  - multifunctional power steering wheel  - Optional navigation system with at least a 7" high-resolution color touch screen resolutions.  - Travel computer with at least 4" high-resolution color screen. Active info screen - basic  - Front fog lights and stop light.  - Heating of the rear window with an electric heater  - The vehicle must be equipped with an FM radio system, MP-3 bluetooth with RDS with AUX and USB connections.  - Rubber floor mats for the entire vehicle  - The vehicle must be branded with built-in sound and light signaling  - Vehicle color: White |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **All items** | **Delivery** of all items to following address: Ministry of Interior, SIV 1, Bulevar Mihajla Pupina 2, Novi Beograd, Republic of Serbia. |  |  |  |
| **All items** | **Testing** of all basic functions of the instrument on a set of producers standard samples commonly used for the corresponding instrument.  Installed equipment must be tested as system, compatible with existing system. |  |  |  |
| **All items** | Technical documentation for equipment (Operating manuals/ Users Guide/ Equipment operating instructions/ Cleaning procedures/ Maintenance procedures/ Calibration procedures) upon delivery. |  |  |  |
| **All items** | **Warranty**  Warranty period 365 days from the issuance of PAC (Provisional Acceptance Certificate) in accordance with article 32 SC and GC of the Contract. Offer must include warranty service description including:   * Service organisation contact data including name, postal address, telephone number, fax number and e-mail address; * Guaranteed that any requests for services will be attended to within 48 hours; * Guarantee that all items can be repaired or alternatively replaced within a maximum of 7 days; * Letter of confirmation that genuine spare parts and consumables will be available for a period of minimum 3 years from the date of final acceptance of the equipment. |  |  |  |
| **All items** | **Commercial warranty**  365 days from the issuance of FAC (Final Acceptance Certificate) in accordance with the conditions laid down in Article 32 of the General Conditions and Article 33 of the Special Conditions.  Detailed description of the organisation of the proposed service and description of the Manufacturer’s commercial warranty shall be included in the offer. |  |  |  |