# *ANNEX II + III:* TECHNICAL SPECIFICATIONS + TECHNICAL OFFER

**Contract title: Electric vehicle p 1 /…**

**Publication reference: RORS00250/City of Zrenjanin/TD2**

**Columns 1-2 should be completed by the contracting authority**

**Columns 3-4 should be completed by the tenderer**

**Column 5 is reserved for the evaluation committee**

Annex III - the contractor's technical offer

The tenderers are requested to complete the template on the next pages:

* Column 2 is completed by the contracting authority shows the required specifications (not to be modified by the tenderer),
* Column 3 is to be filled in by the tenderer and must detail what is offered (for example the words ‘compliant’ or ‘yes’ are not sufficient)
* Column 4 allows the tenderer to make comments on its proposed supply and to make eventual references to the documentation

The eventual documentation supplied should clearly indicate (highlight, mark) the models offered and the options included, if any, so that the evaluators can see the exact configuration. Offers that do not permit to identify precisely the models and the specifications may be rejected by the evaluation committee.

The offer must be clear enough to allow the evaluators to make an easy comparison between the requested specifications and the offered specifications.

| **1.**  **Item number** | **2.**  **Specifications required** | **3.**  **Specifications offered** | **4.**  **Notes, remarks,  ref to documentation** | **5.**  **Evaluation committee’s notes** |
| --- | --- | --- | --- | --- |
| **1** | **Passenger vehicle car: 1 piece**  Description and purpose of vehicle: passenger vehicle suitable for city driving   * Engine type: Electric * Max engine power: min 300 kW * Combined range in line with factory specifications: min 450km * Fast DC charging capability * Steering wheel : Servo on the left side * Cabin type: 4 doors, 5 seats * Vehicle category: M1 * AC device * Cruise control * Minimal safety equipment: 2x airbag, ABS, ESP, hill start assist, parking assistance, automatic pedestrian protection (by breaking or manuvering) * Recognition of traffic signs * 18 inch wheels or larger * Color black, white, gray or other if approved by Contracting Authority prior delivery |  |  |  |