# *ANNEX II + III:* TECHNICAL SPECIFICATIONS + TECHNICAL OFFER

**Contract title: Supply of Cargo Van – Banat Honey Route p 1 /6**

**Publication reference:** RORS00240/ACACSCB/TD4

**Columns 1-2 should be completed by the contracting authority**

**Columns 3-4 should be completed by the tenderer**

**Column 5 is reserved for the evaluation committee**

Annex III - the contractor's technical offer

The tenderers are requested to complete the template on the next pages:

* Column 2 is completed by the contracting authority shows the required specifications (not to be modified by the tenderer),
* Column 3 is to be filled in by the tenderer and must detail what is offered (for example the words ‘compliant’ or ‘yes’ are not sufficient)
* Column 4 allows the tenderer to make comments on its proposed supply and to make eventual references to the documentation

The eventual documentation supplied should clearly indicate (highlight, mark) the models offered and the options included, if any, so that the evaluators can see the exact configuration. Offers that do not permit to identify precisely the models and the specifications may be rejected by the evaluation committee.

The offer must be clear enough to allow the evaluators to make an easy comparison between the requested specifications and the offeredspecifications.

| **1.**  **Item number** | **2.**  **Specifications required** | **3.**  **Specifications offered** | **4.**  **Notes, remarks,  ref to documentation** | **5.**  **Evaluation committee’s notes** |
| --- | --- | --- | --- | --- |
| **1** | **Cargo Van – for Banat Honey Route – 1 piece** |  |  |  |
|  | The vehicle will be used for the transport of materials, beekeeping equipment and up to 2 persons in mixed urban–rural environments. |  |  |  |
|  | **General functional requirements**   * Utility closed-body cargo van, approx. 3.5t GVW (Gross Vehicle Weight) * Suitable for intensive transport and rural operations * Compliant with Romanian homologation rules * Local after-sales service required (at least one service point in Romania) |  |  |  |
|  | **Engine & performance**   * Diesel engine * Emission standard: Euro 6 or higher * Power: minimum 95 kW * Transmission: manual, minimum 6 speeds * Traction: front-wheel drive or equivalent * Combined consumption: ≤ 10 L/100 km (WLTP) * Maximum speed: ≥ 130 km/h |  |  |  |
|  | **Dimensions & capacity**   * External length: maxim 7.00 m * Cargo volume: ≥ 13 m³ * Cargo compartment interior height: minimum 1850 mm (1.85 m) * Maximum authorized mass: 3,300–3,500 kg * Sliding right side door + rear double doors (270° opening) * Seating: minimum 2 persons |  |  |  |
|  | **Safety and standards**   * ABS, ESP, ASR * Driver + passenger airbag * Hill Start Assist * Emergency braking assist * Daytime running lights * Rear-view camera or parking assistance * Tires suitable for all seasons or mixed environments * Homologation and safety compliance with EU standards (UNECE / equivalent) |  |  |  |
|  | **Comfort & cabin equipment**  Minimum:   * Air conditioning * Electric front windows * Central locking with remote * 12V socket(s) in cabin * Adjustable driver seat (height and lumbar) * Infotainment with touchscreen + Bluetooth connectivity * USB charging ports |  |  |  |
|  | **Cargo area requirements**   * Anti-slip wooden or composite floor (or alternative proposal) * Side-wall protective panels (metal or durable composite) * Minimum 6 cargo anchor points * Strong interior lighting (LED or equivalent) |  |  |  |
|  | **Wheels, tyres & suspension**   * Minimum 16" steel wheels * Suspension suitable for mixed road conditions * Tyres:   + Either one full set of all-season tyres OR   + Two sets of tyres (summer + winter) meeting EU standards * Full-size spare wheel included |  |  |  |
|  | **Tools, towing & accessories**   * Jack, wheel wrench, safety triangle, first aid kit * Mandatory: towing hook ("cui de andocare" / trailer hitch) * Must support standard trailer connection per national regulations * Complete manufacturer toolset; * Vehicle to be equipped with a rear tail lift suitable for cargo loading and unloading. |  |  |  |
|  | **Warranty**  Minimum:   * 3 years or 100,000 km full warranty * Spare parts availability: 5 years |  |  |  |
|  | **Delivery conditions**   * Delivery location: Reșița, Romania (beneficiary address) * Delivery deadline: maximum 4 weeks * Vehicle delivered fully homologated and registered * Conformity and inspection certificate required at delivery |  |  |  |