# *ANNEX II + III:* TECHNICAL SPECIFICATIONS + TECHNICAL OFFER

**Contract title: Vehicle with trailer p 1 /…**

**Publication reference: RORS127/Municipality of Bela Crkva/TD5**

**Columns 1-2 should be completed by the contracting authority**

**Columns 3-4 should be completed by the tenderer**

**Column 5 is reserved for the evaluation committee**

Annex III - the contractor's technical offer

The tenderers are requested to complete the template on the next pages:

* Column 2 is completed by the contracting authority shows the required specifications (not to be modified by the tenderer),
* Column 3 is to be filled in by the tenderer and must detail what is offered (for example the words ‘compliant’ or ‘yes’ are not sufficient)
* Column 4 allows the tenderer to make comments on its proposed supply and to make eventual references to the documentation

The eventual documentation supplied should clearly indicate (highlight, mark) the models offered and the options included, if any, so that the evaluators can see the exact configuration. Offers that do not permit to identify precisely the models and the specifications may be rejected by the evaluation committee.

The offer must be clear enough to allow the evaluators to make an easy comparison between the requested specifications and the offered specifications.

| **1.**  **Item number** | **2.**  **Specifications required** | **3.**  **Specifications offered** | **4.**  **Notes, remarks,  ref to documentation** | **5.**  **Evaluation committee’s notes** |
| --- | --- | --- | --- | --- |
| **1** | **Off-road vehicle: 1 piece**  Description and purpose of vehicle: Pickup cargo/passenger vehicle with off road capability   * Max engine power: min 160HP * Max engine torque: min 360Nm * Engine displacement: max. 2000 ccm (cm3) * Engine type: diesel, EURO VI or better * Transmission: 4WD * Steering wheel : Servo on the left side * Ground clearance: min 240mm * Vehicle approach angle forward: min 30o * Vehicle approach angle backward: min 24o * Cabin type: 4 doors * Vehicle category: N1 * Trailer towing force min. 3500 kg * AC device * Minimal safety equipment: 6x airbag, ABS, ESP, TCS, automatic recognition of traffic signs. * 18 inch steel wheels or larger * Equipment obligatory by Serbian traffic legislation. * Color: white, gray or other if previously approved by Contracting Authority |  |  |  |
| **2** | **Vehicle trailer – 1pc**  Description and purpose of trailer: single or double axle trailer to be towed by off-road vehicle capable to carry standard wheeled waste container 1,1m3 made from plastic weighting up to 400kg   * Made from weather resistant metal/material * Metal sides from all sides sufficiently high to secure waste container during transport with back side capable to be lowered and/or tilted for loading/unloading waste container. * With all certificates/accessories/equipment to be road ready and/or registered for traffic in line with Serbian legislation included. |  |  |  |