# *ANNEX II + III:* TECHNICAL SPECIFICATIONS + TECHNICAL OFFER

**Contract title: Procurement of Pick-up vehicle for project Green-Path**

**p 1 /…**

**Publication reference:** **RORS00127-PP2 - TD09**

**Columns 1-2 should be completed by the contracting authority**

**Columns 3-4 should be completed by the tenderer**

**Column 5 is reserved for the evaluation committee**

Annex III - the contractor's technical offer

The tenderers are requested to complete the template on the next pages:

* Column 2 is completed by the contracting authority shows the required specifications (not to be modified by the tenderer),
* Column 3 is to be filled in by the tenderer and must detail what is offered (for example the words ‘compliant’ or ‘yes’ are not sufficient)
* Column 4 allows the tenderer to make comments on its proposed supply and to make eventual references to the documentation

The eventual documentation supplied should clearly indicate (highlight, mark) the models offered and the options included, if any, so that the evaluators can see the exact configuration. Offers that do not permit to identify precisely the models and the specifications may be rejected by the evaluation committee.

The offer must be clear enough to allow the evaluators to make an easy comparison between the requested specifications and the offeredspecifications.

**General Requirements**

* All requirements stated and outlined in this document must be regarded as mandatory and the minimum acceptable criteria. All requirements outlined in this document are accompanied by the phrase "or equivalent".
* The tenderer is required to provide the specifications of the offered items in the Technical Offer, including details such as the manufacturer, product type, model. All documentation must be provided in English or Serbian, both in hardcopy and electronic formats.
* The selected contractor is required to provide all necessary documentation for the registration of the trailer in accordance with the relevant legal regulations in the Republic of Serbia.

| **1.**  **Item number** | **2.**  **Specifications required** | **3.**  **Specifications offered** | **4.**  **Notes, remarks,  ref to documentation** | **5.**  **Evaluation committee’s notes** |
| --- | --- | --- | --- | --- |
| **1** | **Terrain vehicle, Quantity: 1 Unit** |  |  |  |
|  | **Required technical characteristics:**  **VEHICLE SPECIFICATION**  - Year of manufacture: min. 2024  - Seating areas: min. 5  - Engine displacement: min. 1990–2000 cm³  - Engine power: min. 170  - Drive axle: 4x4  - Euro standard: min. EURO VI  - Maximum trailer weight with brakes: min. 3.300 kg  - Gearbox: min. Automatic 10 degrees + reverse or manual 6+1  - Total length: min. 5300 mm  - Total height: min.1800 mm  - Total width: min. 1900 mm  - Maximum length of cargo area: min. 1550 mm  - Cargo space depth: min. 500 mm  - Maximum width of the cargo area: min. 1550–1600 mm  - Cargo space between the wheel arches: min. 1100–1250 mm  -Wheelbase: min. 3200 mm  -Clearance: min. 215 mm  -Maximum trailer weight with brakes: min. 3300 kg  - Approach angle (empty): min. 27°  - Departure angle (empty): min. 25°  - Depth of water hazard: min. 750 mm  VEHICLE EQUIPMENT  - Front and side AirBags for the driver and front passenger, AirBag for the driver's knees  - ABS + ESP  - Electric front and rear windows  - Front and rear fog lights  - Remote central locking  - Automatic dual-zone climate control  - Tempomat  - minimum 12" display with navigation, remote controls on the steering wheel, USB/iPod connection  - BlueTooth  - Tow hitch  - Electrically adjustable, folding mirrors with heaters and lighting  - Metal protection of the undercarriage and tank  - Rear differential lock  - Cargo area lining with integrated 12V socket  - Roof racks  - LED headlights, taillights and fog lights  - 4 cameras – 360 degrees  - Key and keyless vehicle start  - Vehicle entry thresholds  ADDITIONAL REQUIREMENTS  Service interval: min. 15.000 km / 1 year |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **All items** | **Delivery** of all items to following address: Provincial Secretariat for Urban Planning and Environmental Protection, Bulevar Mihajla Pupina, 16, 21101 Novi Sad, Republic of Serbia. |  |  |  |
| **All items** | **Testing** of all basic functions of the instrument on a set of producers standard samples commonly used for the corresponding instrument.  Installed equipment must be tested as system, compatible with existing system. |  |  |  |
| **All items** | Technical documentation for equipment (Operating manuals/ Users Guide/ Equipment operating instructions/ Cleaning procedures/ Maintenance procedures/ Calibration procedures) upon delivery. |  |  |  |
| **All items** | **Warranty**  Warranty period 365 days from the issuance of PAC (Provisional Acceptance Certificate) in accordance with article 32 SC and GC of the Contract. Offer must include warranty service description including:   * Service organisation contact data including name, postal address, telephone number, fax number and e-mail address; * Guaranteed that any requests for services will be attended to within 48 hours; * Guarantee that all items can be repaired or alternatively replaced within a maximum of 7 days; * Letter of confirmation that genuine spare parts and consumables will be available for a period of minimum 3 years from the date of final acceptance of the equipment. |  |  |  |
| **All items** | **Commercial warranty**  365 days from the issuance of FAC (Final Acceptance Certificate) in accordance with the conditions laid down in Article 32 of the General Conditions and Article 33 of the Special Conditions.  Detailed description of the organisation of the proposed service and description of the Manufacturer’s commercial warranty shall be included in the offer. |  |  |  |

**<Signature of authorised representative of the legal entity >**

**< Name and position of authorised representative of the legal entity >**

**< Date >**