# *ANNEX II + III:* TECHNICAL SPECIFICATIONS + TECHNICAL OFFER

**Contract title: Supply of Info totems with software p 1 /…**

**Publication reference: RORS00013/SBPB Vrsac/TD5**

**Columns 1-2 should be completed by the contracting authority**

**Columns 3-4 should be completed by the tenderer**

**Column 5 is reserved for the evaluation committee**

Annex III - the contractor's technical offer

The tenderers are requested to complete the template on the next pages:

* Column 2 is completed by the contracting authority shows the required specifications (not to be modified by the tenderer),
* Column 3 is to be filled in by the tenderer and must detail what is offered (for example the words ‘compliant’ or ‘yes’ are not sufficient)
* Column 4 allows the tenderer to make comments on its proposed supply and to make eventual references to the documentation

The eventual documentation supplied should clearly indicate (highlight, mark) the models offered and the options included, if any, so that the evaluators can see the exact configuration. Offers that do not permit to identify precisely the models and the specifications may be rejected by the evaluation committee.

The offer must be clear enough to allow the evaluators to make an easy comparison between the requested specifications and the offered specifications.

| **1.**  **Item number** | **2.**  **Specifications required** | **3.**  **Specifications offered** | **4.**  **Notes, remarks,  ref to documentation** | **5.**  **Evaluation committee’s notes** |
| --- | --- | --- | --- | --- |
| **1** | **Info totems with software – 5pcs**  **Technical information:**  **Totems:**  **Capacitive touch screen:**   * Multi-functional min 10-point simultaneous touch screen * Screen size: 42” - 52” * Screen resolution: supported 1920 x 1080 * Anti vandal protection glass   **Processing unit:**   * Processor model: min 4 cores 2.6GHz * Ram memory: min 8GB DDR4 * Hard disk: min 128GB SSD or NVME * Operative system: Windows 11 Pro or equivalent/better   **Output Peripherals:**   * Minimum or better - USB 2.0 x 2 connectors, Internet LAN input connector, WiFi antenna integrated into the device. * Minimum or better - 2x3W speakers.   **Dimensions:**   * Weight: less than 50kg, * Height: 180-190cm, * Width: 60-70cm, * Thickness: 5-8cm   **Material:**   * The housing made of sheet steel with reinforcements. * Ventilation and cooling is integrated in housing. Overheating protection implemented in the device.   **Software:**   * The software developed for the totems needs to be visually appealing, user-friendly and its contents must be verified by the CA. It will mostly contain information about the project, information regarding dementia and mental illnesses and other relevant segments. * The Contractor is obliged to maintain and update the software and containing information for the duration of the contract and for the duration of the warranty period. * The CA will provide the contractor with the information needed to be presented through the totems. * All of the content and the visual aspect of the software should be made in accordance with the Visibility manual of the EU, which may be found at the INTERREG IPA CBC Romania Serbia programme website: http://www.romania-serbia.net/ and approved by Contracting Authority. |  |  |  |
|  |  |  |  |  |