# *ANNEX II + III:* TECHNICAL SPECIFICATIONS + TECHNICAL OFFER

**Contract title: Vehicles for medical services p 1 /…**

**Publication reference: RORS00191/DZP/TD3**

**Columns 1-2 should be completed by the contracting authority**

**Columns 3-4 should be completed by the tenderer**

**Column 5 is reserved for the evaluation committee**

Annex III - the contractor's technical offer

The tenderers are requested to complete the template on the next pages:

* Column 2 is completed by the contracting authority shows the required specifications (not to be modified by the tenderer),
* Column 3 is to be filled in by the tenderer and must detail what is offered (for example the words ‘compliant’ or ‘yes’ are not sufficient)
* Column 4 allows the tenderer to make comments on its proposed supply and to make eventual references to the documentation

The eventual documentation supplied should clearly indicate (highlight, mark) the models offered and the options included, if any, so that the evaluators can see the exact configuration. Offers that do not permit to identify precisely the models and the specifications may be rejected by the evaluation committee.

The offer must be clear enough to allow the evaluators to make an easy comparison between the requested specifications and the offered specifications.

| **1.**  **Item number** | **2.**  **Specifications required** | **3.**  **Specifications offered** | **4.**  **Notes, remarks,  ref to documentation** | **5.**  **Evaluation committee’s notes** |
| --- | --- | --- | --- | --- |
| **1** | **Passenger vehicle car: 4 pieces**  Description and purpose of vehicle: small passenger vehicle suitable for city driving   * Max engine power: min 55 kW * Max engine torque: min 115Nm * Engine displacement: max. 2000 ccm (cm3) * Engine type: petrol or diesel or hybrid, EURO VI or better * Fuel consumption in line with factory specification for combined drive: less than 5.5 liters/100km * Steering wheel : Servo on the left side * Cabin type: 4 doors, 5 seats * Vehicle category: M1 * AC device * Cruise control * Start Stop system * Minimal safety equipment: 4x airbag, ABS, ESP, hill start assist, parking sensors on rear, * Recognition of traffic signs for speed limit, STOP, one-way street and prohibited overtaking * 16 inch steel wheels or larger * Color red, white, gray or other if approved by Contracting Authority prior delivery |  |  |  |
| **2** | **Passenger vehicle van: 1 piece**  Description and purpose of vehicle: passenger van suitable for transportation of 8 passengers   * Max engine power: min 130 kW * Max engine torque: min 390Nm * Engine displacement: max. 2000 ccm (cm3) * Engine type: diesel or hybrid, EURO VI or better * Fuel consumption in line with factory specification for combined drive: less than 7 liters/100km * Steering wheel : Servo on the left side * Cabin type: 2 doors at front and sliding door on right side of vehicle, 9 seats * Vehicle category: M1 * AC device * Cruise control * Start Stop system * Minimal safety equipment: 4x airbag, ABS, ESP, hill start assist, parking sensors on rear, * 17 inch steel wheels or larger * Color red, white, gray or other if approved by Contracting Authority prior delivery |  |  |  |