# *ANNEX II + III:* TECHNICAL SPECIFICATIONS + TECHNICAL OFFER

**Contract title: Procurement of Fire truck and Firefighting equipment for project FIREGUARD**

**p 1 /…**

**Publication reference:** **RORS00061–LP–TD03**

**LOT no.2 - Firefighter equipment**

**Columns 1-2 should be completed by the contracting authority**

**Columns 3-4 should be completed by the tenderer**

**Column 5 is reserved for the evaluation committee**

Annex III - the contractor's technical offer

The tenderers are requested to complete the template on the next pages:

* Column 2 is completed by the contracting authority shows the required specifications (not to be modified by the tenderer),
* Column 3 is to be filled in by the tenderer and must detail what is offered (for example the words ‘compliant’ or ‘yes’ are not sufficient)
* Column 4 allows the tenderer to make comments on its proposed supply and to make eventual references to the documentation

The eventual documentation supplied should clearly indicate (highlight, mark) the models offered and the options included, if any, so that the evaluators can see the exact configuration. Offers that do not permit to identify precisely the models and the specifications may be rejected by the evaluation committee.

The offer must be clear enough to allow the evaluators to make an easy comparison between the requested specifications and the offeredspecifications.

**General Requirements**

• All requirements stated and outlined in this document must be regarded as mandatory and the minimum acceptable criteria. All requirements outlined in this document are accompanied by the phrase "or equivalent".

• The tenderer is required to provide the specifications of the offered items in the Technical Offer, including details such as the manufacturer, product type, model, and country of origin. All documentation must be provided in English or Serbian, both in hardcopy and electronic formats.

| **1.**  **Item number** | **2.**  **Specifications required** | **3.**  **Specifications offered** | **4.**  **Notes, remarks,  ref to documentation** | **5.**  **Evaluation committee’s notes** |
| --- | --- | --- | --- | --- |
| **1** | **Protective uniform, Quantity: 35 Units** |  |  |  |
|  | **Required technical characteristics:**  Protective uniforms - three-layer fire suit with CE certificate |  |  |  |
| **2** | **Fireman's knapsack, Quantity: 35 Units** |  |  |  |
|  | **Required technical characteristics:**  Fireman's knapsacks complete with class A pump, TYPE 1, 25 liter volume |  |  |  |
| **3** | **Flail, Quantity: 35 Units** |  |  |  |
|  | **Required technical characteristics:**  Flails - Spring sheet, wooden handles, total length min 200cm |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **All items** | **Delivery** of all items to following address: Forest Estate „Banat“ Pančevo, Republic of Serbia. |  |  |  |
| **All items** | **Testing** of all basic functions of the instrument on a set of producers standard samples commonly used for the corresponding instrument.  Installed equipment must be tested as system, compatible with existing system. |  |  |  |
| **All items** | Technical documentation for equipment (Operating manuals/ Users Guide/ Equipment operating instructions/ Cleaning procedures/ Maintenance procedures/ Calibration procedures) upon delivery. |  |  |  |
| **All items** | **Warranty**  Warranty period 365 days from the issuance of PAC (Provisional Acceptance Certificate) in accordance with article 32 SC and GC of the Contract. Offer must include warranty service description including:   * Service organisation contact data including name, postal address, telephone number, fax number and e-mail address; * Guaranteed that any requests for services will be attended to within 48 hours; * Guarantee that all items can be repaired or alternatively replaced within a maximum of 7 days; * Letter of confirmation that genuine spare parts and consumables will be available for a period of minimum 3 years from the date of final acceptance of the equipment. |  |  |  |
| **All items** | **Commercial warranty**  365 days from the issuance of FAC (Final Acceptance Certificate) in accordance with the conditions laid down in Article 32 of the General Conditions and Article 33 of the Special Conditions.  Detailed description of the organisation of the proposed service and description of the Manufacturer’s commercial warranty shall be included in the offer. |  |  |  |

**<Signature of authorised representative of the legal entity >**

**< Name and position of authorised representative of the legal entity >**

**< Date >**